* Blank page for table of contents
* Design process
* Description of game
* Analysis of strategies
* Selection of strategy
* Analysis of multiple designs
* Selection of design
* Design
* Log
  + Chainbar (5/19)
  + Horizontal claw (5/19)
  + Tested stacking (5/19) works
  + Test defense cone and goal strats (5/22)
  + Build 4 bar
  + Test first mogo lift 4bar (5/26) tilts a lot
  + Reinforce 4 bar
  + Test new 4 bar (5/27) reinforced but still leans, gets on 20 bar but only on
  + Build 3rd 4 bar - taller
  + Test 4 bar (5/28) can get over and drop off
  + Wheels on base
  + Combine subsystems (6/4) no claw
  + Test lifting mogo (6/4)
  + Add claw (6/6)
  + Finish 1st complete robot (6/7)
  + Test chainbar (6/8) bent axles
  + Replace axles
  + Add slew-rate control code, add rubber bands
  + Add screws to claw (6/8) still horizontal
  + Switch to vertical claw
  + Teaser (6/10) test stacking – drops a lot and not as fast as expected
  + Add rubber band cone alignment
  + Practice Stacking (6/13)
  + Modify Screw placement on claw (6/13) 3 per side
  + Test more (6/14)
  + Starting in size
  + Mover claw further forward – standoffs
  + Add c-channel cone alignment
  + Test (6/15)
  + Adjust mogo fork spacing
  + Test zone scoring & stationary goal scoring (6/15)
  + Check driving over bar c-channels and new sizing restriction (6/16)
  + Edit reveal (6/16)
  + Look at righting cones (6/27)
  + Test autoloader (8/2) not much faster
  + Reasoning for new mogo lift (problems and objectives)
  + Begin trying new mogo lift (8/4) above wheels, 1:7, offset horizontal 4bar
  + Test offset 4 bar and realize flipping past issue (8/5)
  + Build singe chainbar in center for mogo (8/12)
  + Test mogo chainbar (8/16) tilts too much
  + Complete current 4bar
  + Test current 4 bar
  + Braydon leaves (8/28)
  + Adjust claw placement, raise and widen chainbar, and change ratio to 3:7 (9/16) some earlier
  + Test and refine placement
  + Tilt mobile goal
  + Switch to rollers (10/9)
  + Confirm work
  + Current wider rollers (10/10)
  + Test rollers and move claw out
  + Refine chain tension
  + Test whole robot (10/22)
  + Rubber bands to prevent getting stuck (10/28)
  + Program auton (10/29)